Advent of Code

--- Day 23: Category Six ---

   The droids have finished repairing as much of the ship as they can. Their report indicates that this was a Category 6
   disaster - not because it was that bad, but because it destroyed the stockpile of Category 6 network cables as well as most
   of the ship's network infrastructure.

   You'll need to rebuild the network from scratch.

   The computers on the network are standard Intcode computers that communicate by sending packets to each other. There are 50
   of them in total, each running a copy of the same Network Interface Controller (NIC) software (your puzzle input). The
   computers have network addresses 0 through 49; when each computer boots up, it will request its network address via a single
   input instruction. Be sure to give each computer a unique network address.

   Once a computer has received its network address, it will begin doing work and communicating over the network by sending and
   receiving packets. All packets contain two values named X and Y. Packets sent to a computer are queued by the recipient and
   read in the order they are received.

   To send a packet to another computer, the NIC will use three output instructions that provide the destination address of the
   packet followed by its X and Y values. For example, three output instructions that provide the values 10, 20, 30 would send a
   packet with X=20 and Y=30 to the computer with address 10.

   To receive a packet from another computer, the NIC will use an input instruction. If the incoming packet queue is empty,
   provide -1. Otherwise, provide the X value of the next packet; the computer will then use a second input instruction to
   receive the Y value for the same packet. Once both values of the packet are read in this way, the packet is removed from the
   queue.

   Note that these input and output instructions never block. Specifically, output instructions do not wait for the sent packet
   to be received - the computer might send multiple packets before receiving any. Similarly, input instructions do not wait for
   a packet to arrive - if no packet is waiting, input instructions should receive -1.

   Boot up all 50 computers and attach them to your network. What is the Y value of the first packet sent to address 255?

   Your puzzle answer was 19530.

--- Part Two ---

   Packets sent to address 255 are handled by a device called a NAT (Not Always Transmitting). The NAT is responsible for
   managing power consumption of the network by blocking certain packets and watching for idle periods in the computers.

   If a packet would be sent to address 255, the NAT receives it instead. The NAT remembers only the last packet it receives;
   that is, the data in each packet it receives overwrites the NAT's packet memory with the new packet's X and Y values.

   The NAT also monitors all computers on the network. If all computers have empty incoming packet queues and are continuously
   trying to receive packets without sending packets, the network is considered idle.

   Once the network is idle, the NAT sends only the last packet it received to address 0; this will cause the computers on the
   network to resume activity. In this way, the NAT can throttle power consumption of the network when the ship needs power in
   other areas.

   Monitor packets released to the computer at address 0 by the NAT. What is the first Y value delivered by the NAT to the
   computer at address 0 twice in a row?

   Your puzzle answer was 12725.

   Both parts of this puzzle are complete! They provide two gold stars: **

   At this point, all that is left is for you to admire your Advent calendar.

   If you still want to see it, you can get your puzzle input.

References

   Visible links
   . https://adventofcode.com/
   . https://adventofcode.com/2019/about
   . https://adventofcode.com/2019/events
   . https://adventofcode.com/2019/settings
   . https://adventofcode.com/2019/auth/logout
   . Advent of Code Supporter
	https://adventofcode.com/2019/support
   . https://adventofcode.com/2019
   . https://adventofcode.com/2019
   . https://adventofcode.com/2019/support
   . https://adventofcode.com/2019/sponsors
   . https://adventofcode.com/2019/leaderboard
   . https://adventofcode.com/2019/stats
   . https://adventofcode.com/2019/sponsors
   . https://en.wikipedia.org/wiki/Category_6_cable
   . https://adventofcode.com/2019/day/9
   . https://en.wikipedia.org/wiki/Blocking_(computing)
   . https://adventofcode.com/2019
   . https://adventofcode.com/2019/day/23/input
